|  |  |
| --- | --- |
| Module | Marionette DAQ |
| Inputs | * USB Power * USB OTG * SPI Network * I2C Network * CAN Network * ADC * Digital Input * UART/USART * Walwart power supply 12V -> 5V * Ethernet |
| Outputs | * SPI Network * I2C Network * CAN Network * ADC * Digital output * UART/USART * USB OTG * Ethernet |
| Funcationality | Multifunction data acquisition device |