Devices needed for selection:

1. LDO
   1. 5.0V in
   2. 3.3V out
2. SPS
   1. 5.0V in
   2. 3.3V out
3. ULPI phy (see figure 89 STM32F407i datasheet)
   1. http://www.digikey.com/product-detail/en/TUSB1210BRHBR/296-28384-1-ND/2627248
      1. Needs 24 or 26MHz crystal
      2. USB HS connector
4. Ethernet phy (see figure 91 and figure 92 STM43F407i datasheet)
   1. RJ-45 Ethernet connector?
   2. Phy 10/100
   3. 50MHz Oscilator
5. Edge connectors
6. USB FS connector
   1. Mini?
   2. Macro?
7. Power input barrel jack
8. SDIO memory card interface?